	.section/PM program0;
	.global _start;
_start:
	/* Type 8: Compute + Dreg move */
	/* AR = AX0 + AY0, MX0 = AX1 */
	ar = ax0 + ay0, ax0 = mx0;

	/* MR = MX0 * MY0 (SS), AX1 = AY0 */
	mr = mx0 * my0 (ss), ax1 = ay0;

	/* NONE = AX0 + AY0 (generate status only) */
	none = ax0 + ay0;

	nop;
_halt:
	jump _halt;
